**SOP FOR NERAC FIT TEST MACHINES RETURN TO SERVICE**

**Please follow the following steps:**

1. **Flush the twin tube with Isopropyl Alcohol several times, let air dry.**
2. **Disinfect the Scott adapter with Fresh Gear (diluted) and let dry**
3. **Using disinfectant wipes wipe down all surfaces on the fit test machine**
4. **Complete inventory of unit**
5. **Leave bag open for 24 hours**

**F drive NERAC /Fit test (Ed S 7-3-2020)**